

EXAMPLE

|  |
| --- |
| **INSPECTION** **and** **TEST** **-** **REPORT****FORMWORK** |
| Contract:Client: Checklist Ref.: | Lot No.: Location: | **Lot** **Opened:** |
| **Lot** **Closed:**Name: |
| **Comments:** *(Delays/Disruption,Improvements,Other)* | Signature: |
|  |
|  |
|  |
| **No.** | **Process** | **Spec/Std/Dwg** | **Acceptance** **Criteria** | **Pass** | **Fail** | **CAR** **Ref:** | **Initial(ITP)** | **Date** |
| 1 | Subcontractor Review |  |  |  |  |  |  |  |
| 2 | Safety Induction |  |  |  |  |  |  |  |
| 3 | Approve Shop Drawings, design calculationsand use of proprietary deck and perimeter systems. |  |  |  |  |  |  |  |
| 4 | Check Setout for:. R.L.. Corner point location.. Penetrations.. Construction joints. | AS 3600, AS3610. |  |  |  |  |  |  |
| 5 | Check Falsework for:. Plumb. Bracing. Soffit R.L.. Set down.. Fillets. Joints. To Approved Plans/Design.. Notification to Client for final inspection. | AS 3600, AS3610. |  |  |  |  |  |  |
| 6 | FINAL INSPECTION (Including review of Items 3 to 5 above). Check as follows:1. Forms (plumb and braced).
2. Core holes and embedments.
3. Inserts, anchor bolts and holding down bolts.
4. Chamfers and grooves.
5. Wall and column forms (through temporary openings).
 |  |  |  |  |  |  |  |
| 7 | Monitor stripping and backpropping. |  |  |  |  |  |  |  |
| 8 | FINAL INSPECTION (Including review of Item 7above). | AS 3600, AS3610. |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
| **Note:** **Ensure** **all** **certificates,** **records** **and** **photos** **are** **attached** **to** **the** **Inspection** **Report** |

Page 1 of 1