EXAMPLE

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **INSPECTION and TEST - REPORT**  **STRUCTURAL STEEL** | | | | | | | | |
| Contract:  Client: Checklist Ref.: | | Lot No.:    Location: | | | | **Lot Opened:** | | |
| **Lot Closed:**  Name: | | |
| **Comments:** *(Delays/Disruption,Improvements,Other)* | | | | | | Signature: | | |
|  | | | | | | | | |
|  | | | | | | | | |
|  | | | | | | | | |
| **No.** | **Process** | **Spec/Std/Dwg** | **Acceptance Criteria** | **Pass** | **Fail** | **CAR Ref:** | **Initial(ITP)** | **Date** |
| 1 | Subcontractor Review |  |  |  |  |  |  |  |
| 2 | Safety Induction |  |  |  |  |  |  |  |
| 3 | Approve Shop Drawings |  |  |  |  |  |  |  |
| 4 | Approve welding procedures. |  |  |  |  |  |  |  |
| 5 | Obtain Welders Certificates or arrange tests for  Welders. |  |  |  |  |  |  |  |
| 6 | Check set out. |  |  |  |  |  |  |  |
| 7 | Monitor Welding |  |  |  |  |  |  |  |
| 8 | Non-Destructive tests on welded joints by: (Select according to specification.)   * Radiographic methods. * Ultrasonic methods. * Magnetic particle testing media. * Penetrant (dye type) testing media. |  |  |  |  |  |  |  |
| 9 | Check fabricated members. |  |  |  |  |  |  |  |
| 10 | Monitor painting and/or special coating. |  |  |  |  |  |  |  |
| 11 | Test paint and/or special coating. |  |  |  |  |  |  |  |
| 12 | FINAL INSPECTION - (Including review of  records for Items 3 to 11 above). |  |  |  |  |  |  |  |
| 13 | Check deliveries of steelwork to site. |  |  |  |  |  |  |  |
| 14 | Check set out. |  |  |  |  |  |  |  |
| 15 | Check holding down bolts and bearing plates. |  |  |  |  |  |  |  |
| 16 | Monitor site welding. |  |  |  |  |  |  |  |
| 17 | Non-Destructive tests on site welded joints by: (Select according to specification.)   * Radiographic methods. * Ultrasonic methods. * Magnetic particle testing media. * Penetrant (dye type) testing media. |  |  |  |  |  |  |  |
| 18 | Check erected steelwork as follows:   1. Steel members. 2. Splices and joints. 3. Bolts, nuts, washers and packers. 4. Wedging under base plates. |  |  |  |  |  |  |  |
| 19 | Obtain Regulatory Authorities' Certificates and  Approvals. |  |  |  |  |  |  |  |
| 20 | Obtain guarantees. |  |  |  |  |  |  |  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **No.** | **Process** | **Spec/Std/Dwg** | **Acceptance Criteria** | **Pass** | **Fail** | **CAR Ref:** | **Initial(ITP)** | **Date** |
| 21 | Inspections  . Commencement of shop fabrication.  . Commencement of welding procedure tests.  . Commencement of welding.  . Prior to placement of root rung of complete penetration butt welds.  . Completion of fabrication prior to surface preparation.  . Commencement of surface preparation prior to protective coating.  . Completion of protective coating prior to site delivery.  . Steelwork on site prior to erection.  . Completion of erection prior to encasing or fixing cladding.  . Encasing |  |  |  |  |  |  |  |
| 22 | Check structural steel plumbed and braced. |  |  |  |  |  |  |  |
| 23 | Check base plates grouted. |  |  |  |  |  |  |  |
| 24 | FINAL INSPECTION - (Including review of records for Items 13 to 23 above.) Check grouting to bases and touching up  primer/coatings. |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
| **Note: Ensure all certificates, records and photos are attached to the Inspection Report** | | | | | | | | |