EXAMPLE

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **INSPECTION and TEST - REPORT**  **RENDER** | | | | | | | | |
| Contract:  Client: Checklist Ref.: | | Lot No.:    Location: | | | | **Lot Opened:** | | |
| **Lot Closed:**  Name: | | |
| **Comments:** *(Delays/Disruption,Improvements,Other)* | | | | | | Signature: | | |
|  | | | | | | | | |
|  | | | | | | | | |
|  | | | | | | | | |
| **No.** | **Process** | **Spec/Std/Dwg** | **Acceptance Criteria** | **Pass** | **Fail** | **CAR Ref:** | **Initial(ITP)** | **Date** |
| 1 | Subcontractor Review |  |  |  |  |  |  |  |
| 2 | Safety Induction |  |  |  |  |  |  |  |
| 3 | Approve samples. |  |  |  |  |  |  |  |
| 4 | Check deliveries of materials as follows:   1. Cement and lime. 2. Fine aggregate.   (a) Cement and lime. |  |  |  |  |  |  |  |
| **OR**  Polymer based render |
| 5 | Check substrate. |  |  |  |  |  |  |  |
| 6 | Approve sample panels of render. |  |  |  |  |  |  |  |
| 7 | Check beads, lathing, etc. |  |  |  |  |  |  |  |
| 8 | Check set-out of control joints. |  |  |  |  |  |  |  |
| 9 | Monitor rendering:   1. Mixing 2. Application |  |  |  |  |  |  |  |
| 10 | Check rendered surfaces:   1. Finished Surfaces 2. Control Joints |  |  |  |  |  |  |  |
| 11 | Obtain warranties. |  |  |  |  |  |  |  |
| 12 | FINAL INSPECTION - (Including review of  records for Items 3 to 11 above). |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
| **Note: Ensure all certificates, records and photos are attached to the Inspection Report** | | | | | | | | |

Page 1 of 1